1. Vacuum well has to be spaced very closely (1 to 2.5 m).
2. Distance between rows of well should not be more than 15m to 20m.